**Zoostliss FTTH Fiber Optic Tool Kit**

Portable optical power meter is an accurate and durable handheld meter designed for the installation, operation and maintenance of optical fiber network. It is a compact device with backlight switch and auto power on-off ability. Besides, it provides ultra-wide measurement range, high accuracy, user self-calibration function and universal port. In addition, it displays linear indicators (mW) and non-linear indicators (dBm) in one screen at the same time.

**Brief Specifications:**

* **Wavelength(nm):** 800~1700nm
* **Detector:** InGaAs
* **Measurement Range (dBm):** -70~+10
* **Uncertainty:** ±0.2(5%)
* **Calibrated Wavelength(nm):** 850,980,1300,1310,1490,1550
* **Resolution(dB): Linear indication:** 0.1%
* **Loharithmic indication:** 0.01dBm
* **Optical Connector:** FC/ Universal 2.5mm adaptor
* **Operating Temperature:** -10 ~ +60C
* **Storage Temperature:** -25 ~ +70C
* **Relative Humidity:** 0 to 95% (non-condensing)

