**Beam 280**

|  |  |
| --- | --- |
| **280-2.jpg** | **280w-1.jpg** |
| **Lamp Type:** | Moving Head Lights | **Lamp Inside:** | **MSD 10R** |
| **Working Temperature:** | 15-45 | **Color Temperature:** | **8000K** |
| **Lamp Power(W):** | 280W | **Input Voltage(V):** | 100-240V |
| **Colour:** **Gomo:** | 14 Colors + open**17 Gobos + open** | **Channel Mode:** | 16 Channel |
| **Packing Size:** | **590\*370\*390mm** | **Net Weight:** | 16.5kg |